[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Addresses Excluded from DHCP Local Server Use

#### Purpose

Display addresses that have been excluded by the ip dhcp-local excluded-address command. The DHCP local server does not allocate excluded addresses, because they are already used by devices on the subnetwork.

#### Action

To display excluded IP addresses:

    host1(config)#show ip dhcp-local excluded
         Dhcp Excluded Addresses
         -----------------------
                  Low         High
      Pool      Address     Address
    --------   ---------   ----------
    default    10.10.1.1
    default    10.10.1.5   10.10.1.30
    cable2     10.10.2.1
    home.com   10.10.3.1
    cable4     10.10.4.1
    cable5     10.10.5.1

#### Meaning

Table 100 lists the show ip dhcp-local excluded command output fields.

Table 100: show ip dhcp-local excluded Output Fields

Field Name | Field Description
--- | ---
Pool | Name of the pool that contains the excluded address
Low Address | Excluded address or first address in a range of addresses
High Address | Last address in a range of addresses

#### Related Topics

- show ip dhcp-local excluded

[Contents] [Prev] [Next] [Index] [Report an Error]