[Contents] [Prev] [Next] [Index] [Report an Error]

# neighbor ibgp-singlehop

#### Syntax

[ no | default ] neighbor { ipAddress | ipv6Address | peerGroupName } ibgp-singlehop

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Configures an internal BGP peer to be a single-hop (non-multihop) peer. The no version restores the default, wherein internal peer cannot be a single hop. The default version removes the explicit configuration from the peer or peer group and reestablishes inheritance of the feature configuration.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command, unless it is overridden for a specific peer.

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]