[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting the Excess Burst for a Rate-Limit Profile

For one-rate rate-limit profiles only, use the excess-burst command to set the excess burst in bytes for a rate-limit profile; range is 0–4294967295. Use the excess-burst command to set the excess burst in milliseconds for a rate-limit profile; range is 1–10000. The no version restores the default value, 0.

- Issue the excess-burst command from Rate Limit Profile Configuration mode:
  `
  host1(config-rate-limit-profile)#excess-burst millisecond 1000
  `

#### Related Topics

- excess-burst

[Contents] [Prev] [Next] [Index] [Report an Error]