[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dvmrp metric-offset

#### Syntax

[ no ] ip dvmrp metric-offset { in | out } [ increment ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Adjusts the number of hops associated with routes passing through an interface. This action indicates that the route is more efficient or less efficient than an alternative route. The no version restores the default values.

#### Options

- in—Increments the number of hops for a DVMRP route advertised in incoming DVMRP reports. If you do not specify a key word, this option is the default.
- out—Increments the number of hops for a DVMRP route advertised in outgoing DVMRP reports
- increment—Number of hops associated with this interface; default value is 1 for incoming reports and 0 for outgoing reports.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]