[Contents] [Prev] [Next] [Index] [Report an Error]

# vlan service-profile

#### Syntax

[ no ] vlan service-profile profileName

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Assigns an IP service profile to a VLAN subinterface. The service profile must be defined in the default virtual router. The no version removes the IP service profile from the VLAN subinterface.

#### Options

- profileName—Name of the IP service profile

#### Mode

Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]