[Contents] [Prev] [Next] [Index] [Report an Error]

# show l2tp dial-out target

#### Syntax

show l2tp dial-out target [ targetIpAddress targetIpAddressMask | allVirtualRouters ]
[ detail ] [ state operState ] [ filter ]

To display summary information:

show l2tp dial-out target summary [ allVirtualRouters ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays configured dial-out targets within the current virtual router context.

#### Options

- targetIpAddress—Trigger IP address for the target that you want to display
- targetIpAddressMask—Mask for the trigger IP address
- allVirtualRouters—Displays dial-out information for all virtual routers
- detail—Displays configuration, state, and statistics
- operState—One of the following operational states:
  - down
  - inService
  - inhibited
- filter—See Filtering show Commands
- summary—Displays aggregate counts for targets in each of the possible operational and administrative states

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]