[Contents] [Prev] [Next] [Index] [Report an Error]

# sscc transportRouter

#### Syntax

sscc transportRouter name

no sscc transportRouter [ name ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the router on which the TCP/COPS connection is to be established. The no version removes the SRC client transport router.

#### Options

- name—Name of a transport router

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]