[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring SRC Client Connection Statistics

#### Purpose

Display statistics about connection between the SRC client and SAE. The command output refers to the SRC client by its former name, SSC client.

#### Action

To display statistics for the SRC client connection:

    host1#show sscc statistics
    SSC Client Statistics:
            Policy Commands received   0
            Policy Commands(List)      0
            Policy Commands(Acct)      0
            Bad Policy Cmds received   0
            Error Policy Cmds received 0
            Policy Reports sent        3
            Connection attempts        7
            Connection Open requests   7
            Connection Open completed  0
            Connection Closed sent     0
            Connection Closed remotely 5
            Create Interfaces sent     0
            Delete Interfaces sent     3
            Active IP Interfaces       3282
            IP Interface Transitions   3281
            Synchronizes received      0
            Synchronizes rcvd & droped 0
            Synchronize Complete sent  2
            Internal Errors            0
            Communication Errors       0
            Discovers Seen             15263
            Active Discovers           4911
            Discover Transitions       20704
            Discover Creates Sent      15263
            Discover Deletes Sent      10352
            Active Addresses           3274
            Address Transitions        3280
            Create Addresses Sent      3277
            Delete Addresses Sent      3

#### Meaning

Table 30 lists the show sscc statistics command output fields.

Table 30: show sscc statistics Output Fields

Field Name | Field Description
--- | ---
Policy Commands received | Number of policy commands received on the SRC client connection
Policy Commands(List) | Number of Policy Commands with subtype List
Policy Commands(Acct) | Number of Policy Commands with subtype Accounting
Bad Policy Cmds received | Number of Policy Commands received with bad policies
Error Policy Cmds received | Number of Policy Commands received with errors
Policy Reports sent | Number of Policy Reports sent
Connection Open requests | Number of connections the SRC client has tried to open with a remote SAE
Connection Open completed | Number of connections successfully open to the SAE
Connection Closed sent | Number of connections the SRC client has closed
Connection Closed remotely | Number of connections that were closed by the remote SAE
Create Interfaces sent | Number of create interface indications sent to the SAE
Delete Interfaces sent | Number of delete interface indications sent to the SAE
Active IP Interfaces | Current number of active IP interfaces the SRC client is aware of
IP Interface Transitions | Number of IP interface transitions logged by the SRC client
Synchronizes received | Number of synchronization requests the SRC client received from the SAE
Synchronize Complete sent | Number of synchronization complete indications sent
Internal Errors | Number of internal errors
Communication Errors | Number of errors with lower-layer communications (such as socket errors)

#### Related Topics

- show sscc statistics

[Contents] [Prev] [Next] [Index] [Report an Error]