[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring LDP Targeted Hello Receive and Send Lists

Purpose

Display LDP targeted hello receive or send list, or both.

Action

To display both the LDP targeted hello receive and send lists:

    host1#show ldp targeted session
    Mpls Target Session Status:

     D = Dynamically, S = Statically, A = Access List Configured

        Targeted session sent to 10.9.1.3 is up  Used By: D
          indirect nexthop index 3, resolved
        Targeted session sent to 10.9.1.6 is up  Used By: S
          indirect nexthop index 206, resolved

Meaning

Table 41 lists the show ldp targeted session command output fields.

Table 41: show ldp targeted session Output Fields

Field Name | Field Description
--- | ---
D | Targeted session created by layer 2 over MPLS connection; see Layer 2 Services over MPLS Overview in the JUNOSe BGP and MPLS Configuration Guide for more information about layer 2 over MPLS
S | Targeted session statically created by user
A | Targeted session created by access list
Used By | Letter representing source of targeted session

#### Related Topics

- show ldp targeted session

[Contents] [Prev] [Next] [Index] [Report an Error]