[Contents] [Prev] [Next] [Index] [Report an Error]

# ip ospf authentication-none

#### Syntax

ip ospf authentication-none

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that no authentication is to be used for the interface. The no version has no effect.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]