[Contents] [Prev] [Next] [Index] [Report an Error]

# graceful-restart helper

#### Syntax

[ no ] graceful-restart helper

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the router to function as an OSPFv2 or OSPFv3 graceful restart helper router. The no version disables OSPF graceful restart helper mode capability on the router.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]