[Contents] [Prev] [Next] [Index] [Report an Error]

# Removing PIM

To remove PIM from a VR, use the no ipv6 router pim command.

ipv6 router pim

- Use to create and enable PIM processing on a VR or to access Router Configuration mode.
- Example
  `
  host1:boston(config)#no ipv6 router pim
  `
- Use the no version to remove PIM from the VR.
- See ipv6 router pim.

[Contents] [Prev] [Next] [Index] [Report an Error]