[Contents] [Prev] [Next] [Index] [Report an Error]

# clear bridge

#### Syntax

clear bridge { bridgeGroupName | vplsName }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
vplsName variable added in JUNOSe Release 7.1.0.

#### Description

Removes all dynamic (learned) MAC address entries from the forwarding table for the specified bridge group or VPLS instance . There is no no version.

#### Options

- bridgeGroupName—Name of a bridge group specified with the bridge command
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command

#### Mode

Privileged Exec

#### Related Topics

- Clearing Dynamic MAC Addresses from the VPLS Forwarding Table in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]