[Contents] [Prev] [Next] [Index] [Report an Error]

## isisNsfEvents

#### Description

Log events related to IS-IS non-stop forwarding procedure during system warm start

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

Logs IS-IS NSF timer related events (for example, expiration and cancellation of timers [T1, T2, T3])

#### Debug

Restart-request transmit; restart-ack receive; SNP receive processing; LSP synchronization; LSP purging

#### Filter 1

interface—See description of the isisAdjChange interface filter for information about this filter

#### Filter 2

router—See description of the isisAdjChange router filter for information about this filter

[Contents] [Prev] [Next] [Index] [Report an Error]