[Contents] [Prev] [Next] [Index] [Report an Error]

# radius pppoe nas-port-format unique

#### Syntax

[ no ] radius pppoe nas-port-format unique

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Allows the E-series RADIUS client to use a unique value for the NAS-Port attribute for subscribers on PPPoE interfaces. The router derives the unique value from the subscriber’s profileHandle. The no version restores the default value, determined by the interface.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]