[Contents] [Prev] [Next] [Index] [Report an Error]

# ip vrrp enable

#### Syntax

[ no ] ip vrrp vrid [ enable ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables a VRID. The no version disables a VRID. The default is disabled.

#### Options

- vrid—VRID identifier; a number in the range 1–255

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]