[Contents] [Prev] [Next] [Index] [Report an Error]

# graceful-restart restart-time

#### Syntax

[ no ] graceful-restart restart-time restartTime

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the estimated time for the restarting OSPFv2 router to reacquire OSPF neighbors that were fully functional prior to the restart. When this timer expires, the restarting router exits the restart procedure, originates any LSAs that were suppressed during the restart, removes any self-originated LSAs that it received from helping neighbors, runs SPF, and updates any routes in the routing table. The no version returns the restart duration timer to its default value, 180 seconds.

#### Options

- restartTime—Number of seconds during which the restarting router can reacquire OSPF neighbors that were fully functional prior to the restart; in the range 1–1800

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]