[Contents] [Prev] [Next] [Index] [Report an Error]

## isisAdjChange

#### Description

IS-IS adjacency up or down

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

Adjacency state change

#### Info

None

#### Debug

None

#### Filter 1

interface interfaceType interfaceSpecifier

- interface—Logs events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

#### Filter 2

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- interface—Logs events on a specific interface on the virtual router
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]