[Contents] [Prev] [Next] [Index] [Report an Error]

# clns holding-time

#### Syntax

clns holding-time holdTime

no clns holding-time

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Allows the sender of an ES hello or IS hello to specify the length of time you consider the information in the hello packets to be valid. The no version restores the default value, 30 seconds.

#### Options

- holdTime—Number in the range 1–65535; length of time in seconds during which the information in the hello packets is considered valid

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]