[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Virtual Router Groups Configured for AAA Broadcast Accounting

#### Purpose

Display the virtual router groups that are configured for AAA broadcast accounting.

For additional information about the show configuration command, see JUNOSe System Basics Configuration Guide.

#### Action

To display the virtual router groups that are configured for AAA broadcast accounting:

    host1#show configuration category aaa global-attributes
    ! Configuration script being generated on MON JAN 10 2005 15:19:19 UTC
    ! Juniper Edge Routing Switch ERX-1440
    ! Version: 9.9.9 development-4.0 (January 7, 2005  17:26)
    ! Copyright (c) 1999-2004 Juniper Networks, Inc.  All rights reserved.
    !
    ! Commands displayed are limited to those available at privilege level 15
    !
    ! NOTE:  This script represents only a subset of the full system configuration.
    ! The category displayed is: aaa global-attributes
    !
    aaa accounting vr-group groupXyzCompany10
     aaa virtual-router 1 vrXyzA
     aaa virtual-router 2 vrXyzB
     aaa virtual-router 3 vrXyzC
     aaa virtual-router 4 vrXyzD

    aaa accounting vr-group groupXyzCompany20
     aaa virtual-router 1 vrXyzP
     aaa virtual-router 2 vrXyzQ
     aaa virtual-router 3 vrXyzR
     aaa virtual-router 4 vrXyzS
    !
    hostname "host1"

#### Meaning

Table 18 lists the show configuration category aaa global-attributes command output fields.

Table 18: show configuration category aaa global-attributes Output Fields

Field Name | Field Description
--- | ---
aaa accounting vr-group | Name of virtual router groups
aaa virtual-router | Name and index number of the virtual routers that are members of the virtual router group

#### Related Topics

- show configuration category aaa global-attributes

[Contents] [Prev] [Next] [Index] [Report an Error]