[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa route-download

#### Syntax

aaa route-download [ downloadInterval ] [ retry-interval retryInterval ]
[ cost cost ] [ tag tagValue ] [ base-user-name name ] [ password password ]
[ synchronization time ]

no aaa route-download

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Enables the RADIUS route-download server and configures parameters for the server. The no version disables the route-download server.

#### Options

- downloadInterval—Interval between download operations, in the range 1–1440 minutes; default is 720 minutes
- retryInterval—Interval between retries after a failed download, in the range 1–60 minutes; default is 10 minutes
- cost—Default cost of a downloaded route, in the range 1–254; default is 2
- tagValue—Default tag of a downloaded route, in the range 1–4294967295; default is 0
- name—Name of router used for route-download requests; default is the router hostname
- password—Password used for route-download requests
- time—Time the download operation is restarted each day, in 24-hour format (hh:mm:ss)

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]