[Contents] [Prev] [Next] [Index] [Report an Error]

# radius ethernet-port-type

#### Syntax

radius ethernet-port-type [ virtual | ethernet ]

no radius ethernet-port-type

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Indicates to RADIUS which Ethernet port type to use in RADIUS attribute 61, NAS-Port-Type, for all Ethernet users on the E-series router. The no version restores the default, ethernet.

#### Options

- virtual—Sets RADIUS NAS-Port-Type to virtual
- ethernet—Sets RADIUS NAS-Port-Type to Ethernet

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]