[Contents] [Prev] [Next] [Index] [Report an Error]

# show subscribers

#### Syntax

To display detailed information:

show subscribers [ ipv6 [ ipv6Prefix ] ]
[ domain domainName | interface { atm | ethernet } interfaceSpecifier |
port interfaceSpecifier | slot slotNumber | username userName |
virtual-router vrName ] [ filter ]

To display summary information:

show subscribers summary [ domain | interface | port | slot | virtual-router ]
[ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
interface, atm, and ethernet keywords added in JUNOSe Release 7.3.0.
slot keyword and slotNumber variable added in JUNOSe Release 7.3.0.

#### Description

Displays the active subscribers on your router.

#### Options

- ipv6—Displays IPv6 subscribers for the domain
- ipv6Prefix—Prefix that defines the IPv6 network that you want to filter
- userName—Username of active subscriber
- domain—Displays active subscribers for the domain
- domainName—Domain name matching usernames of active subscribers
- interface—Displays active subscribers for the the specified interface, atm or ethernet, or in the summary version, displays active subscribers for all ATM and Ethernet interfaces
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- port—Displays active subscribers for the port
- slot—Displays active subscribers for the slot
- slotNumber—Number of the chassis slot of the line module in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), 0–13 (ERX14xx models), 0-5 (E120 router), and 0-16 (E320 router)
- virtual-router—Displays active subscribers for the VR
- vrName—Name of the VR to which interfaces of active subscribers are bound
- filter—See Filtering show Commands
- summary—Displays the active subscribers for each domain, interface, port, slot, or virtual router

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]