[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Locked Out Destinations

#### Purpose

Display information about the L2TP destinations that are currently locked out.

#### Action

To display information about the L2TP destinations that are currently locked out:

    host1#show l2tp destination lockout
    L2TP destination 36 is waiting for lockout timeout (45 seconds remaining)
    L2TP destination 54 is waiting for lockout test start
    L2TP destination 76 is waiting for lockout test complete
    3 L2TP lockout destinations found

#### Meaning

Table 84 lists the show l2tp destination lockout command output fields.

Table 84: show l2tp destination lockout Output Fields

Field Name | Field Description
--- | ---
L2TP destination waiting | Name of destination and its lockout status. The status indicates whether the destination is waiting for the lockout timeout to expire (and how much time is left), or waiting for the lockout test to start or finish
L2TP lockout destinations found | Number of destinations that are currently in lockout state

#### Related Topics

- show l2tp destination lockout

[Contents] [Prev] [Next] [Index] [Report an Error]