[Contents] [Prev] [Next] [Index] [Report an Error]

# profile vlan bulk-config

#### Syntax

profile vlan bulk-config bulkConfigName profileName

no profile vlan bulk-config bulkConfigName

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Assigns the base profile configured for a dynamic VLAN subinterface to the VLAN range configured on a static VLAN major interface with the vlan bulk-config command. The no version removes the base profile assignment.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- profileName—Profile name of up to 80 characters

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]