[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rip copy-to-dynamic

#### Syntax

[ no ] ip rip copy-to-dynamic

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables RIP on dynamic, unnumbered IP interfaces. You cannot configure RIP on dynamic interfaces directly. However, this command allows dynamic, unnumbered interfaces (that refer to numbered IP interface for configuration data) to obtain RIP attributes from the numbered IP interface to which they refer. The no version disables the feature but does not remove all existing, active RIP interfaces that were created by this command.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]