[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls backup-path

#### Syntax

[ no ] mpls [ traffic-eng ] backup-path bypassTunnelName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns the specified bypass tunnel to the interface that you want to protect. The no version removes the assignment.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- bypassTunnelName—Name of the bypass tunnel

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]