[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Secure Policy Lists

#### Purpose

Display information about only secure policy lists. This command and the output are visible only to authorized users—the mirror-enable command must be enabled before using this command. Use the name keyword to display information for a specific secure policy list.

#### Action

To display information about secure policy lists:

    host1#show secure policy-list

                                      Policy Table
                                      ------ -----
    Secure IP Policy secureIpPolicy
       Administrative state: enable
       Reference count:      2
       Classifier control list: secClassA
          mirror analyzer-ip-address 192.168.1.1 analyzer-virtual-router default analyzer-udp-port 3000 mirror-id 6789 session-id 6543

       Referenced by interface(s):
          ATM5/0.1  secure-input policy, statistics disabled, virtual-router default
          ATM5/0.1  secure-output policy, statistics disabled, virtual-router default

    Secure IPv6 Policy secure-ipv6-pol3
       Administrative state: enable
       Reference count:      2
       Classifier control list: *
          Mirror analyzer-ip-address 190.168.1.1 analyzer-virtual-router default analyzer-udp-port 3000 mirror-id 6789 session-id 6543

       Referenced by interface(s):
          GigabitEthernet1/0/2.1.2  secure-input policy, statistics disabled, virtual-router default
          GigabitEthernet1/0/2.1.2  secure-output policy, statistics disabled, virtual-router default

       Referenced by merged policies:
          None

    L2TP Secure Policy secureL2tpPolicy
       Administrative state: enable
       Reference count:      2
       Classifier control list: *
          mirror analyzer-ip-address 192.168.2.1 analyzer-virtual-router default analyzer-udp-port 3000 mirror-id 6789 session-id 6543 (unreachable)

       Referenced by interface(s):
          TUNNEL l2tp:1/msn.pwh.com/1  secure-input policy, statistics disabled
          TUNNEL l2tp:1/msn.pwh.com/1  secure-output policy, statistics disabled

#### Meaning

Table 67 lists show secure policy-list command output fields.

Table 67: show secure policy-list Output Fields

Field Name | Field Description
--- | ---
Policy | Type (IP, IPv6, or L2TP) and name of the policy list
Administrative state | Status of administrative state, enable or disable; set to enable when the policy list is created
Reference count | Number of attachments to interfaces or profiles
Classifier control list | Name of the classifier control list
Mirror analyzer-ip-address | IP address of analyzer device
Analyzer-virtual-router | Analyzer interface virtual router
Analyzer-udp-port | UDP port used to communicate with analyzer device
Mirror-id | Unique identifier of the mirrored session
Session-id | Unique identifier of the user session
Referenced by interface(s) | List of interfaces to which the policy is attached; indicates whether the attachment is at secure input or secure output of interface
Referenced by profile(s) | Not currently supported: always null
Statistics | Not currently supported: always disabled

#### Related Topics

- show secure policy-list

[Contents] [Prev] [Next] [Index] [Report an Error]