[Contents] [Prev] [Next] [Index] [Report an Error]

# gre destination profile

#### Syntax

gre destination profile profileName { [ any-virtual-router ] |
[ virtual-router virtualRouterName ] }

no gre destination profile profileName

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Configures a destination profile for dynamic GRE tunnels and enters IP Tunnel Destination Profile Configuration mode. The no version deletes the destination profile.

#### Options

- profileName—Name of the destination profile
- any-virtual-router—Specifies a default destination profile for all virtual routers; only one default destination profile can be defined in the system
- virtualRouterName—Name of the transport virtual router

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]