> - ip analyzer
> - Related Topics
> - Configuring CLI-Based Mirroring
> - Configuring RADIUS-Based Mirroring

> # ip analyzer

> #### Syntax

> ip analyzer [ default ]

> no ip analyzer

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures an interface as an analyzer interface, for use in an interface mirroring configuration. The no version removes the analyzer interface configuration from the interface.

> #### Options

> - default—Specifies that this interface is the default analyzer interface for the virtual router

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.