[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring LDP Profiles

Purpose

Display a specific LDP profile, or all LDP profiles.

Action

To display the default LDP profile:

    host1:pe2#show ldp profile default
    ldp profile default: used by 2 interfaces
       session retry:  10 times at interval 10

| Note: The mpls keyword is optional and is provided for compatibility with non–E Series implementations.

Meaning

Table 39 lists the show ldp profile command output fields.

Table 39: show ldp profile Output Fields

Field Name | Field Description
--- | ---
profile | Number of interfaces that use the profile
session retry | Number of attempts that will be made to set up an MPLS LDP session

#### Related Topics

- show ldp profile

[Contents] [Prev] [Next] [Index] [Report an Error]