[Contents] [Prev] [Next] [Index] [Report an Error]

# How RADIUS Dynamic-Request Server Works

In a typical client-server RADIUS environment, the E Series router functions as the client and the RADIUS server functions as the server. However, when using the RADIUS dynamic-request server feature, the roles are reversed. For example, during a RADIUS-initiated disconnect operation, the E Series router’s RADIUS dynamic-request server functions as the server, and the RADIUS server functions as the disconnect client.

[Contents] [Prev] [Next] [Index] [Report an Error]