> - debounce

> # debounce

> #### Syntax

> debounce [ seconds ]

> no debounce

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Enables the debounce timer and sets the time interval that the interface waits before reporting a state change to the upper-layer protocols. The no version restores the default behavior, disabling debounce on the interface.

> #### Options

> - seconds—Interval for which an interface must maintain a given state before the interface reports the state change to the upper-layer protocols. Number in the range 1–5 seconds; default value is 1 second.

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.