[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 virtual-router

#### Syntax

[ no ] ipv6 virtual-router vrName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies a virtual router in an IPv6 profile. Dynamic interfaces created with the profile are assigned to this VR. The no version removes the VR from the profile; if a VR is not specified via RADIUS, then any subsequent creation process for dynamic interfaces using the profile fails.

#### Options

- vrName—Name of the virtual router; a string of 1–15 alphanumeric characters

#### Mode

Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]