> - Downloads
> - ip vrrp priority

> # ip vrrp priority

> #### Syntax

> ip vrrp vrid priority priorityValue

> no ip vrrp vrid priority

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the priority of VRRP routers. The no version restores the default value, 100.

> #### Options

> - vrid—VRID identifier; a number in the range 1–255
> - priorityValue—Priority value of the VRRP router; a number in the range 1–255; default value is 100

> #### Mode

> Interface Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.