> - Downloads
> - Configuring an ICR Partition
> - Related Topics
> - ICR Overview
> - Monitoring the Configuration of ICR Partitions
> - Monitoring the Configuration of an ICR Partition Attached to an Interface
> - Monitoring the Status of ICR Partition Accounting

> # Configuring an ICR Partition

> When you configure an ICR partition, you configure the interface on which the ICR partition resides and create a unique VRRP instance to manage the partition.

> To configure an ICR partition:

> 1. Configure the interface.

>    See Configuring the Interface on Which the ICR Partition Resides.

> 2. Create a unique VRRP instance to manage the ICR partition.

>    See Configuring VRRP Instances to Match ICR Requirements.

> 3. Create and assign a name to the ICR partition.

>    See Naming ICR Partitions.

> 4. (Optional) Group the subscribers.

>    See Grouping ICR Subscribers Based on S-VLAN IDs and Grouping ICR Subscribers Based on VLAN IDs.

>    | Note: Grouping subscribers based on S-VLAN IDs is the default grouping option for ICR partitions. If you do not explicitly specify the grouping option, subscribers are grouped based on S-VLAN IDs.

> 5. (Optional) Configure RADIUS.

>    See Using RADIUS to Manage Subscribers Logging In to ICR Partitions

> #### Published: 2009-10-07

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.