> - Downloads
> - vlan service-profile

> # vlan service-profile

> #### Syntax

> [ no ] vlan service-profile profileName

> #### Release Information

> Command introduced in JUNOSe Release 7.1.0.

> #### Description

> Assigns an IP service profile to a VLAN subinterface. The service profile must be defined in the default virtual router. The no version removes the IP service profile from the VLAN subinterface.

> #### Options

> - profileName—Name of the IP service profile

> #### Mode

> Profile Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.