[Contents] [Prev] [Next] [Index] [Report an Error]

# green-mark

#### Syntax

[ no ] green-mark colorMarkValue

#### Release Information

Command introduced in JUNOSe Release 7.2.0.

#### Description

Applies ToS mark value to green packets, which can be from policy actions, earlier policies, or rate-limit hierarchies. The no version deletes the ToS mark value.

#### Options

- colorMarkValue—Value of the ToS mark to be applied: in the range 0–255

#### Mode

Color Mark Profile Configuration

#### Related Topics

- Hierarchical Rate Limits Overview
- Policy Rule Precedence

[Contents] [Prev] [Next] [Index] [Report an Error]