> - Downloads
> - subscriber disconnect

> # subscriber disconnect

> #### Syntax

> [ no ] subscriber disconnect

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Enables the E Series router to receive RADIUS-initiated disconnect messages from the RADIUS server. The no version restores the default, in which support for RADIUS-initiated disconnect messages is disabled on the router.

> | Note: This command and the RADIUS dynamic-request server feature replace the radius disconnect client command, which has been deprecated and may be removed completely in a future release. The RADIUS Disconnect Configuration mode has also been deprecated.

> #### Mode

> RADIUS Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.