> - Downloads
> - show configuration

> # show configuration

> #### Syntax

> show configuration [ interface interfaceType interfaceSpecifier ] |
> [ category categoryName [ categoryName ]* ] [ virtual-router routerName ]
> [ [ exclude-category interface interfaceType ]* ] [ include-defaults ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays the current (running) configuration of the router, a specified virtual router, a specified interface, or a specified category of router settings. You can create a configuration script from this output by saving it as a file with the .scr extension. This command was formerly documented as show config; that abbreviation is still supported.

> #### Options

> - interfaceType—Interface type; see Interface Types and Specifiers
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - categoryName—Name of the category or subcategory of router settings; first categoryName variable in the syntax represents the category; repeated categoryName variables represent subcategories of the category
> - routerName—Name of the virtual router
> - exclude-category—Excludes information associated with a particular type of interface
> - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
> - include-defaults—Includes commands that set default values for various parameters
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.