> - Downloads
> - mirror analyzer-ip-address
> - Related Topics
> - Configuring CLI-Based Mirroring

> # mirror analyzer-ip-address

> #### Syntax

> mirror analyzer-ip-address analyzerIpAddress analyzer-virtual-router vrName
> [ analyzer-udp-port udpPort [ mirror-identifier mirrorId
> [ session-identifier sessionId ] ] ]

> no mirror

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the mirror action for a classifier group in a secure IP or L2TP policy list. The no version deletes the mirror rule.

> #### Options

> - analyzerIpAddress—IP address of the analyzer
> - vrName—Name of the virtual router where the analyzer interface is configured
> - udpPort—UDP port of the analyzer; required for L2TP packet mirror rules
> - mirrorId—Mirror identifier
> - sessionId—Session identifier

> #### Mode

> Classifier-Group Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.