[Contents] [Prev] [Next] [Index] [Report an Error]

# disable-incremental-external-spf

#### Syntax

[ no ] disable-incremental-external-spf

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Disables incremental external SPF on the router; results in a full SPF when an event occurs to trigger an external SPF. The no version reenables incremental external SPF.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]