[Contents] [Prev] [Next] [Index] [Report an Error]

# qos-port-type-profile

#### Syntax

qos-port-type-profile typeOfInterface qos-profile qosProfileName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
lag keyword added in JUNOSe Release 8.1.0.

#### Description

Associates a QoS profile with all the ports of a given interface type. There is no no version.

#### Options

- typeOfInterface—One of the following interface types to be associated with the QoS port-type profile; atm, ethernet, lag, serial, server-port
- qosProfileName—Name of the QoS profile

#### Mode

Global Configuration

#### Related Topics

- Attaching a QoS Profile to an Interface
- Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups

[Contents] [Prev] [Next] [Index] [Report an Error]