[Contents] [Prev] [Next] [Index] [Report an Error]

# hops-of-statistics-kept

#### Syntax

hops-of-statistics-kept [ hopsKeptValue ]

no hops-of-statistics-kept

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the number of hops to keep statistics for an entry. The no version restores the default value.

#### Options

- hopsKeptValue—Number of hops for which statistics are collected for a particular pathEcho type; default value is 16 for a pathEcho entry and 1 for an echo entry; if you omit this option, all hops found are recorded

| Note: The E Series router supports only the pathEcho and echo types.

#### Mode

RTR Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]