[Contents] [Prev] [Next] [Index] [Report an Error]

# neighbor advertisement-interval

#### Syntax

neighbor { ipAddress | ipv6Address | peerGroupName } advertisement-interval seconds

no neighbor { ipAddress | ipv6Address | peerGroupName } advertisement-interval
[ seconds ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
ipv6Address variable added in JUNOSe Release 8.0.0.

#### Description

Sets the minimum interval between the sending of BGP updates for a given prefix. The no version restores the default interval.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command, unless it is overridden for a specific peer.
- seconds—Interval in seconds between update messages; in the range 0–600; default value is 30 seconds for external peers and 5 seconds for internal peers

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]