> - Downloads
> - radius ethernet-port-type

> # radius ethernet-port-type

> #### Syntax

> radius ethernet-port-type [ virtual | ethernet ]

> no radius ethernet-port-type

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Indicates to RADIUS which Ethernet port type to use in RADIUS attribute 61, NAS-Port-Type, for all Ethernet users on the E Series router. The no version restores the default, ethernet.

> #### Options

> - virtual—Sets RADIUS NAS-Port-Type to virtual
> - ethernet—Sets RADIUS NAS-Port-Type to Ethernet

> #### Mode

> Global Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.