> - Downloads
> - show l2tp tunnel

> # show l2tp tunnel

> #### Syntax

> show l2tp tunnel [ detail ] [ state { adminState | ifOperStatus |
> failover-resync failoverResyncMode } ]
> [ l2tpName | [ virtual-router vrName ] ip ipAddress [ l2tpNameNoDest ] ] [ filter ]

> To display summary information:

> show l2tp tunnel summary [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> failover-resync keyword and failoverResyncMode variable added in JUNOSe Release 9.0.0.

> #### Description

> Displays detailed information about the configured and operational status of selected L2TP tunnels or summary information for all L2TP tunnels.

> #### Options

> - detail—Provides complete information about the specified sessions, including the L2TP host profile name
> - adminState—Displays information about tunnels only with the specified effective administrative state
>   - enabled—Effective administrative state is disabled
>   - disabled—Effective administrative state is enabled
>   - drain—Effective administrative state is drain
> - ifOperStatus—Displays information about tunnels only with the specified operational state
>   - up—Operational state is up
>   - down—Operational state is down
>   - lower-down— Operational state is lower down
>   - not-present—Operational state is not-present
> - failoverResyncMode—Displays information about tunnels that use the specified failover resynchronization mode:
>   - disable—Peer failover resynchronization is disabled
>   - failover-protocol—Uses the L2TP failover protocol method
>   - failover-protocol-fallback-to-silent-failover—Uses the L2TP failover protocol method; however, if the peer does not support this method, the silent failover method is used
>   - not-configured—Uses the global failover method because peer failover resynchronization is not configured for L2TP host profiles and AAA domain map tunnels
>   - silent-failover—Uses the L2TP silent failover method
> - l2tpName—Tunnel name
> - vrName—Name of the virtual router on which the tunnel exists
> - ipAddress—IP address
> - l2tpNameNoDest—Tunnel name
> - filter—See Filtering show Commands
> - summary—Displays the configured and operational status of all L2TP tunnels

> #### Mode

> Privileged Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.