> - Downloads
> - sscc address

> # sscc address

> #### Syntax

> sscc { primary | secondary | tertiary } address ipAddress [ port portNumber ]

> no sscc { primary | secondary | tertiary } address [ ipAddress [ port portNumber ] ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the SRC client (formerly SSCC) with the IP addresses of the SRC servers and the ports on which the servers listen for activity. The no version removes the specified server (primary, secondary, or tertiary) from the list of SRC servers.

> #### Options

> - primary—Primary SRC server
> - secondary—Secondary SRC server
> - tertiary—Tertiary SRC server
> - ipAddress—IP address of an SRC server
> - portNumber—SRC server port number on which the server listens for activity; default port is 3288

> #### Mode

> Global Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.