> - Downloads
> - show ip route

> # show ip route

> #### Syntax

> show ip route [ vrf vrfName ] [ destination [ ipMask ] [ detail ] ] [ all ] [ protocol ]
> [ filter ]

> To display summary information:

> show ip route summary [ vrf vrfName ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays current state of the routing table.

> #### Options

> - vrfName—Displays the contents of the IP routing table associated with a VRF
> - destination—Specifies the IP address or domain name of the host to show
> - ipMask—IP mask of the specific address to show
> - detail—Displays detailed information about the specific prefix; currently shows the tag added by means of the ip route command
> - all—Displays all routes in the routing table inserted from all protocols (not just the best routes that are used for forwarding)
> - protocol—One of the following protocols for which you want to display the best routes in the routing table; no routes are displayed if routes for the specified protocol are not present in the routing table
>   - access—Displays the best access-server routes (BGP) in the routing table
>   - access-internal—Displays the best access-internal routes in the routing table
>   - bgp—Displays the best BGP routes in the routing table
>   - bgp-tunnel—Displays the best BGP tunnel routes in the routing table
>   - dvmrp—Displays the best DVMRP routes in the routing table
>   - isis—Displays the best IS-IS routes in the routing table
>   - ldp—Displays the best LDP tunnel routes in the routing table
>   - local—Displays the best locally connected routes in the routing table
>   - mbgp—Displays the best MBGP routes in the routing table
>   - ospf—Displays the best OSPF routes owned by in the routing table
>   - other—Displays the best internal control routes in the routing table
>   - rip—Displays the best RIP routes in the routing table
>   - rsvp—Displays the best RSVP tunnel routes in the routing table
>   - static—Displays the best static routes added by network management to the routing table
>   - static-rpf—Displays the best static RPF routes added by network management to the routing table
> - summary—Displays summary counters for all routes in the IP routing table
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec, User Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.