> - Downloads
> - show radius remote-circuit-id-delimiter

> # show radius remote-circuit-id-delimiter

> #### Syntax

> show radius remote-circuit-id-delimiter

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays the delimiter character that the router uses to set off components in the PPPoE remote circuit ID value sent from a DSLAM and captured on the router. The default delimiter character is #.

> #### Mode

> Privileged Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.